(kicad_pcb (version 3) (host pcbnew "(2013-jul-07)-stable")
  (general
    (links 50)
    (no_connects 0)
    (area 199.924999 124.924999 229.075001 162.075001)
    (thickness 1.6)
    (drawings 16)
    (tracks 143)
    (zones 0)
    (modules 31)
    (nets 17)
  )
  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.889)
    (via_drill 0.6)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.2)
    (mod_text_size 1.5 1.5)
    (mod_text_width 0.15)
    (pad_size 5.00126 5.00126)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF39)
    (pcbplotparams
      (layerselection 284196865)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber_Starter_Kit/))
  )
  (net 0 "")
  (net 1 +1.5V)
  (net 2 +3.3V)
  (net 3 +4.5V)
  (net 4 /GPIO0_1)
  (net 5 /GPIO0_2)
  (net 6 /GPIO0_3)
  (net 7 /GPIO0_5)
  (net 8 DGND)
  (net 9 N-0000010)
  (net 10 N-0000011)
  (net 11 N-0000013)
  (net 12 N-0000014)
  (net 13 N-0000015)
  (net 14 N-000002)
  (net 15 "UART RX")
  (net 16 UART_TX)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.6)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net /GPIO0_1)
    (add_net /GPIO0_2)
    (add_net /GPIO0_3)
    (add_net /GPIO0_5)
    (add_net N-0000010)
    (add_net N-0000011)
    (add_net N-0000013)
    (add_net N-0000014)
    (add_net N-0000015)
    (add_net N-000002)
    (add_net "UART RX")
    (add_net UART_TX)
  )
  (net_class Power ""
    (clearance 0.25)
    (trace_width 0.508)
    (via_dia 0.889)
    (via_drill 0.6)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +1.5V)
    (add_net +3.3V)
    (add_net +4.5V)
    (add_net DGND)
  )
  (module TH4_e1.27mm_d0.5mm_LED (layer F.Cu) (tedit 523C0A24)
    (at 214.2998 154.2288 270)
    (clearance 0.2)
    (fp_text reference D1 (at -0.7874 1.41732 270) (layer F.SilkS))
    (fp_text value LED_RGB_4PINS (at -0.72136 1.4732 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 N-0000013)
    )
    (pad 4 thru_hole circle (at -2.54 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 13 N-0000015)
    )
    (pad 1 thru_hole circle (at 1.27 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 12 N-0000014)
    )
  )
  (module TH2_e2mm_d0.5mm_R (layer F.Cu) (tedit 52385659)
    (at 222.23984 128.08712 55)
    (fp_text reference R3 (at 0 3.10896 55) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 -2.89052 55) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 55) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 UART_TX)
    )
    (pad 2 thru_hole circle (at 2 0 55) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 N-000002)
    )
  )
  (module TH2_e2mm_d0.5mm_R (layer F.Cu) (tedit 5238511F)
    (at 210.27644 145.923 160)
    (fp_text reference R1 (at 0 3.10896 160) (layer F.SilkS) hide)
    (fp_text value 100k (at 0 -2.89052 160) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 160) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /GPIO0_5)
    )
    (pad 2 thru_hole circle (at 2 0 160) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V)
    )
  )
  (module TH2_e2mm_d0.5mm_R (layer F.Cu) (tedit 52385200)
    (at 212.71992 148.02104 270)
    (fp_text reference R8 (at 0 3.10896 270) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 -2.89052 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 13 N-0000015)
    )
    (pad 2 thru_hole circle (at 2 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 +4.5V)
    )
  )
  (module TH2_e2mm_d0.5mm_R (layer F.Cu) (tedit 52385203)
    (at 215.3158 148.0058 270)
    (fp_text reference R7 (at 0 3.10896 270) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 -2.89052 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 N-0000013)
    )
    (pad 2 thru_hole circle (at 2 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 +4.5V)
    )
  )
  (module TH2_e2mm_d0.5mm_R (layer F.Cu) (tedit 52385206)
    (at 218.1098 146.56308 240)
    (fp_text reference R5 (at 0 3.10896 240) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 -2.89052 240) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 240) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 12 N-0000014)
    )
    (pad 2 thru_hole circle (at 2 0 240) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 +4.5V)
    )
  )
  (module TH2_e2mm_d0.5mm_R (layer F.Cu) (tedit 523850D7)
    (at 220.41104 126.50724 235)
    (fp_text reference R2 (at 0 3.10896 235) (layer F.SilkS) hide)
    (fp_text value 100k (at 0 -2.89052 235) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 235) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 /GPIO0_1)
    )
    (pad 2 thru_hole circle (at 2 0 235) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V)
    )
  )
  (module TH2_e2mm_d0.5mm_R (layer F.Cu) (tedit 5238515C)
    (at 223.56572 132.72008 250)
    (fp_text reference R4 (at 0 3.10896 250) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 -2.89052 250) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 250) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /GPIO0_3)
    )
    (pad 2 thru_hole circle (at 2 0 250) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 N-0000010)
    )
  )
  (module TH2_e2mm_d0.5mm_R (layer F.Cu) (tedit 5238515F)
    (at 223.65716 139.5222 250)
    (fp_text reference R6 (at 0 3.10896 250) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 -2.89052 250) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 250) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 /GPIO0_2)
    )
    (pad 2 thru_hole circle (at 2 0 250) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 N-0000011)
    )
  )
  (module TH2_e1.5mm_d0.5mm_D4mm (layer F.Cu) (tedit 523851A2)
    (at 209.6262 142.494)
    (fp_text reference C1 (at 0 4.0386) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 -4.08432) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -0.75 0) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V)
    )
    (pad 2 thru_hole circle (at 0.75 0) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
  )
  (module SWITCH_CMS (layer F.Cu) (tedit 5238E19A)
    (at 212.852 126.746 180)
    (descr "SURFACE MOUNT MOMENTARY PUSHBUTTON SWITCHES SPST NORMALLY OPEN")
    (tags "SURFACE MOUNT MOMENTARY PUSHBUTTON SWITCHES SPST NORMALLY OPEN")
    (attr smd)
    (fp_text reference SW2 (at 0 -2.4384 180) (layer F.SilkS) hide)
    (fp_text value ISP (at 5.07492 0.72136 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.99974 0 180) (size 1.99898 1.6002)
      (layers F.Cu F.Mask)
      (net 4 /GPIO0_1)
    )
    (pad 2 smd rect (at 2.99974 0 180) (size 1.99898 1.6002)
      (layers F.Cu F.Mask)
      (net 8 DGND)
    )
  )
  (module SWITCH_CMS (layer F.Cu) (tedit 5238E17E)
    (at 213.27364 160.11144)
    (descr "SURFACE MOUNT MOMENTARY PUSHBUTTON SWITCHES SPST NORMALLY OPEN")
    (tags "SURFACE MOUNT MOMENTARY PUSHBUTTON SWITCHES SPST NORMALLY OPEN")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.4384) (layer F.SilkS) hide)
    (fp_text value Reset (at -0.08128 -2.45872) (layer F.SilkS))
    (pad 1 smd rect (at -2.99974 0) (size 1.99898 1.6002)
      (layers F.Cu F.Mask)
      (net 8 DGND)
    )
    (pad 2 smd rect (at 2.99974 0) (size 1.99898 1.6002)
      (layers F.Cu F.Mask)
      (net 7 /GPIO0_5)
    )
  )
  (module PIN_ARRAY_4x1 (layer F.Cu) (tedit 5238AA4E)
    (at 216.95156 143.77924)
    (descr "Double rangee de contacts 2 x 5 pins")
    (tags CONN)
    (clearance 0.24)
    (fp_text reference P1 (at -1.21412 2.27076) (layer F.SilkS))
    (fp_text value CONN_4 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /GPIO0_5)
    )
    (pad 2 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 UART_TX)
    )
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /GPIO0_3)
    )
    (pad 4 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 /GPIO0_2)
    )
    (model pin_array\pins_array_4x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_4x1 (layer F.Cu) (tedit 5238AA78)
    (at 216.99728 130.58648 180)
    (descr "Double rangee de contacts 2 x 5 pins")
    (tags CONN)
    (fp_text reference P2 (at -0.39116 2.01168 180) (layer F.SilkS))
    (fp_text value CONN_4 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 /GPIO0_1)
    )
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V)
    )
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
    (pad 4 thru_hole circle (at 3.81 0 180) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 15 "UART RX")
    )
    (model pin_array\pins_array_4x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mire_Ronde_1mm (layer F.Cu) (tedit 51005D6C)
    (at 201.9808 128.4732)
    (fp_text reference M1 (at 0 -1.75006) (layer F.SilkS) hide)
    (fp_text value MIRE_RONDE (at 0 1.84912) (layer F.SilkS) hide)
    (pad 0 connect circle (at 0 0) (size 1.00076 1.00076)
      (layers F.Cu F.Mask)
    )
  )
  (module Mire_Ronde_1mm (layer F.Cu) (tedit 51005D6C)
    (at 226.6188 158.623)
    (fp_text reference M2 (at 0 -1.75006) (layer F.SilkS) hide)
    (fp_text value MIRE_RONDE (at 0 1.84912) (layer F.SilkS) hide)
    (pad 0 connect circle (at 0 0) (size 1.00076 1.00076)
      (layers F.Cu F.Mask)
    )
  )
  (module Mire_Ronde_1mm (layer F.Cu) (tedit 51005D6C)
    (at 202.1078 158.496)
    (fp_text reference M3 (at 0 -1.75006) (layer F.SilkS) hide)
    (fp_text value MIRE_RONDE (at 0 1.84912) (layer F.SilkS) hide)
    (pad 0 connect circle (at 0 0) (size 1.00076 1.00076)
      (layers F.Cu F.Mask)
    )
  )
  (module TH2_e2.54mm_d0.5mm_D5.9mm_LED (layer F.Cu) (tedit 5238AA6E)
    (at 226.19716 129.29616 90)
    (fp_text reference D2 (at 0.09652 -1.82372 90) (layer F.SilkS))
    (fp_text value LED (at 0.01524 -4.00304 90) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -1.27 0 90) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
    (pad 1 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 N-000002)
    )
  )
  (module TH2_e2.54mm_d0.5mm_D5.9mm_LED (layer F.Cu) (tedit 5238AA69)
    (at 226.20224 136.10844 90)
    (fp_text reference D3 (at 0.0508 -1.7526 90) (layer F.SilkS))
    (fp_text value LED (at 0.01524 -4.00304 90) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -1.27 0 90) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
    (pad 1 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 N-0000010)
    )
  )
  (module TH2_e2.54mm_d0.5mm_D5.9mm_LED (layer F.Cu) (tedit 5238AA59)
    (at 226.20732 142.91056 90)
    (fp_text reference D4 (at 0.07112 -1.87452 90) (layer F.SilkS))
    (fp_text value LED (at 0.01524 -4.00304 90) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -1.27 0 90) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
    (pad 1 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 N-0000011)
    )
  )
  (module TH3_e1.27mm_d0.5_TO92 (layer F.Cu) (tedit 523877B8)
    (at 227.70592 128.03124 270)
    (tags TO92)
    (clearance 0.2)
    (fp_text reference Q1 (at 0 4.74472 270) (layer F.SilkS) hide)
    (fp_text value NPN (at -0.0254 -4.55168 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 N-000002)
    )
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 13 N-0000015)
    )
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
  )
  (module TH3_e1.27mm_d0.5_TO92 (layer F.Cu) (tedit 523877F5)
    (at 227.72624 134.83844 270)
    (tags TO92)
    (clearance 0.2)
    (fp_text reference Q2 (at 0 4.74472 270) (layer F.SilkS) hide)
    (fp_text value NPN (at -0.0254 -4.55168 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 N-0000010)
    )
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 N-0000013)
    )
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
  )
  (module TH3_e1.27mm_d0.5_TO92 (layer F.Cu) (tedit 52387805)
    (at 227.70592 141.63548 270)
    (tags TO92)
    (clearance 0.2)
    (fp_text reference Q3 (at 0 4.74472 270) (layer F.SilkS) hide)
    (fp_text value NPN (at -0.0254 -4.55168 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 N-0000011)
    )
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 12 N-0000014)
    )
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1 1) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
  )
  (module DIP8 (layer F.Cu) (tedit 52387D83)
    (at 216.96172 137.09904)
    (fp_text reference U1 (at -1.5494 0.20828) (layer F.SilkS))
    (fp_text value LPC810M021FN8FP (at 0.01524 -6.6802) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.27 1.27) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /GPIO0_5)
    )
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.27 1.27) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 UART_TX)
    )
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.27 1.27) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /GPIO0_3)
    )
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.27 1.27) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 /GPIO0_2)
    )
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.27 1.27) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 /GPIO0_1)
    )
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.27 1.27) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V)
    )
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.27 1.27) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 DGND)
    )
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.27 1.27) (drill 0.8)
      (layers *.Cu *.Mask F.SilkS)
      (net 15 "UART RX")
    )
  )
  (module Support_Pile_Bouton_11.6mm (layer F.Cu) (tedit 523895AB)
    (at 204.9272 134.1374 90)
    (tags "Support Pile Bouton 12mm")
    (fp_text reference BT2 (at -7.35076 -3.54076 180) (layer F.SilkS))
    (fp_text value BATTERY (at 0.08636 -5.11556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 7.59968 0 90) (size 1.6 1.6) (drill 1.02)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V)
    )
    (pad 1 thru_hole circle (at -7.59968 0 90) (size 1.6 1.6) (drill 1.02)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 +3.3V)
    )
    (pad 2 smd circle (at 0 0.1 90) (size 5.00126 5.00126)
      (layers F.Cu F.Mask)
      (net 1 +1.5V)
      (clearance 2.99974)
    )
  )
  (module Support_Pile_Bouton_11.6mm (layer F.Cu) (tedit 523895A8)
    (at 205.0288 152.908 90)
    (tags "Support Pile Bouton 12mm")
    (fp_text reference BT1 (at 7.24916 -3.51536 180) (layer F.SilkS))
    (fp_text value BATTERY (at 0.08636 -5.11556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 7.59968 0 90) (size 1.6 1.6) (drill 1.02)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +1.5V)
    )
    (pad 1 thru_hole circle (at -7.59968 0 90) (size 1.6 1.6) (drill 1.02)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +1.5V)
    )
    (pad 2 smd circle (at 0 0.1 90) (size 5.00126 5.00126)
      (layers F.Cu F.Mask)
      (net 8 DGND)
      (clearance 2.99974)
    )
  )
  (module Support_Pile_Bouton_11.6mm (layer F.Cu) (tedit 52389706)
    (at 223.70288 152.98928 270)
    (tags "Support Pile Bouton 12mm")
    (fp_text reference BT3 (at -7.19328 2.74828 360) (layer F.SilkS))
    (fp_text value BATTERY (at 0.08636 -5.11556 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 7.59968 0 270) (size 1.6 1.6) (drill 1.02)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 +4.5V)
    )
    (pad 1 thru_hole circle (at -7.59968 0 270) (size 1.6 1.6) (drill 1.02)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 +4.5V)
    )
    (pad 2 smd circle (at 0 0.1 270) (size 5.00126 5.00126)
      (layers F.Cu F.Mask)
      (net 2 +3.3V)
      (clearance 2.99974)
    )
  )
  (module LOGO_TI_BACK_135 (layer B.Cu) (tedit 0)
    (at 206.1972 137.12444)
    (fp_text reference L1 (at 0 -4.48818) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 4.48818) (layer B.SilkS) hide)
  )
  (module tmp_silkscreen-back_13mm_OWF (layer B.Cu) (tedit 0)
    (at 221.9706 154.5082)
    (fp_text reference G*** (at 0 -6.59638) (layer B.SilkS) hide)
    (fp_text value tmp_silkscreen-back_13mm_OWF (at 0 6.59638) (layer B.SilkS) hide)
  )
  (module OSHW_logo_silkscreen-front_7mm (layer B.Cu) (tedit 0)
    (at 205.16596 152.5524)
    (fp_text reference G*** (at 0 -3.71094) (layer B.SilkS) hide)
    (fp_text value OSHW_logo_silkscreen-front_7mm (at 0 3.71094) (layer B.SilkS) hide)
  )
  (module PIN_ARRAY_1 (layer F.Cu) (tedit 523C19F4)
    (at 217.87612 126.19736)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P3 (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value Fixation (at 0 -1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (model pin_array\pin_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Techno-Innov (at 212.17636 128.07696) (layer B.SilkS))
  (gr_text +V (at 218.1606 135.1534 90) (layer B.SilkS))
  (gr_text 0.1 (at 220.91904 135.31088 90) (layer B.SilkS))
  (gr_text 0.2 (at 220.8276 138.92276 90) (layer B.SilkS))
  (gr_text 0.3 (at 218.34856 138.89736 90) (layer B.SilkS))
  (gr_text 0.4 (at 215.8238 138.85164 90) (layer B.SilkS))
  (gr_text 0.5 (at 213.26348 138.8872 90) (layer B.SilkS))
  (gr_text GND (at 215.7222 135.636 90) (layer B.SilkS))
  (gr_text 0.0 (at 213.23808 135.28548 90) (layer B.SilkS))
  (gr_text v0.2 (at 208.7118 134.6962) (layer B.SilkS))
  (gr_text "Starter kit" (at 205.994 132.8166) (layer B.SilkS))
  (gr_text "LPC810\n" (at 207.264 130.7592) (layer B.SilkS))
  (gr_line (start 200 162) (end 200 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 229 162) (end 229 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 162) (end 229 162) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 125) (end 229 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 8) (net_name DGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.26))
    (polygon
      (pts
        (xy 200.0758 125.07468) (xy 228.92512 125.0696) (xy 228.92004 161.91992) (xy 200.07072 161.925)
      )
    )
  )
)
